ekeyBridge and ekeyDevice Drivers for Control4
Version 102 

This package includes:
- ekeybridge.c4z — Driver for project-level integration
- ekeydevice.c4z — Driver for room-level fingerprint and digital input notifications
- Documentation-V102.pdf — Setup and integration guide

Driver Availability
The drivers ekeybridge.c4z and ekeydevice.c4z will be submitted to Control4 for certification.
Once certified, they will be listed in the Control4 online driver database.
Until then, both drivers must be added manually to Composer Pro from this ZIP file.

Adding ekeybridge.c4z to the Project
You can add the ekeybridge driver in two ways, depending on whether the ekeyBridgeC4 device is installed:

1. If the ekeyBridgeC4 device is installed:
   Control4 will automatically discover it using SDDP. The ekeybridge driver will appear under the Discovered tab in Composer Pro.
   - Double-click the discovered device to add it to the project.
   - To access the ekeyBeidgeC4 web interface, go to Connections > Network > Available Devices, then hold Control and click on the SDDP device labeled ekey_<mac_address>.

2. If the ekeyBridgeC4 is not installed:
   - In Composer Pro, open the Items tab.
   - Locate ekeybridge.c4z, and double-click to add it to the project manually.

Adding ekeydevice.c4z to the Project
Add the ekeydevice driver to individual rooms during configuration.
This driver enables fingerprint and digital input notifications for automation at the room level.

Functionality Overview
Use these drivers to integrate ekey bionyx devices (xLine, sLine, dLine) with Control4.
They support up to 14 predefined automation events per room, triggered by fingerprint group matches or digital inputs.

For Setup and Support
Please refer to the included Documentation-V102.pdf for detailed setup instructions.
If you need assistance, contact: support@ekeyusa.com
